gplink-2.1.3 (Mar 12 2018)
Listing File Generated: 2018-5-14  10:58:00
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           #include "mc32p7511.inc"
                                           		LIST
                                           ;mc32p7511.inc    Standard Header File, Version 1.00 by Sinomcu
                                           		NOLIST
                                           
                                                   ORG     0X0000
000000   a001     goto    0x1                      GOTO    START
                                                     
                                                    
                                           START:       
000001   3cfd     movai   0xfd                     MOVAI   0XFd   ;P01输入不上拉
000002   5791     movra   0x191                    MOVRA    OEP0
                                                 
000003   3cff     movai   0xff                     MOVAI   0Xff
000004   5795     movra   0x195                    MOVRA   OEP1        
000005   3c01     movai   0x1                      movai       0x01
000006   57b0     movra   0x1b0                    movra       ADCR0      ;内部参考3V                
000007   3c05     movai   0x5                      movai       0x05
000008   57b1     movra   0x1b1                    movra       ADCR1      ;测内参3V时要开AD ，输出至P01  P01要设为输入不上拉才能测内参 
                                                   ;MOVAI   0X01;高频
                                                   ;nop;MOVAI   0X06;低频
                                                   ;;MOVAI   0X00
                                                   ;nop;MOVRA   OSCM
                                                   ;goto   LOOP
                                                   ;fill 0xa5a5,0x300
                                           LOOP:
                                                    ;CLRWDT
000009   7390     comr    0x190                     COMR   IOP0
00000a   0000     nop                               NOP
00000b   a009     goto    0x9                       GOTO   LOOP
                                                    
                                                    END


MEMORY USAGE MAP ('X' = Used,  '-' = Unused)

0000 : XXXXXXXXXXXXXXXX XXXXXXXX-------- ---------------- ----------------

All other memory blocks unused.

Program Memory Words Used:    12

