gplink-2.1.3 (Mar 12 2018)
Listing File Generated: 2018-5-14  10:58:21
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           #include "mc32p7510.inc"
                                           		LIST
                                           ;mc32p7510.inc    Standard Header File, Version 1.00 by Sinomcu
                                           		NOLIST
                                           
                                                   ORG 0X0000
000000   a001     goto    0x1                      GOTO    START
                                                     
                                                    
                                           START:       
000001   3cff     movai   0xff                     MOVAI   0XFF 
000002   5791     movra   0x191                    MOVRA    OEP0
                                                 
000003   3c00     movai   0                        MOVAI   0X00
000004   5795     movra   0x195                    MOVRA   OEP1
000005   3cff     movai   0xff                     MOVAI   0XFF 
000006   5796     movra   0x196                    MOVRA   PUP1
                                                   ;MOVAI   0X01;¸ßÆµ
                                                   ;nop;MOVAI   0X06;µÍÆµ
                                                   ;;MOVAI   0X00
                                                   ;nop;MOVRA   OSCM
                                                   ;goto   LOOP
                                                   ;fill 0xa5a5,0x300
                                           LOOP:
                                                    ;CLRWDT
000007   7390     comr    0x190                     COMR   IOP0
000008   0000     nop                               NOP
000009   a007     goto    0x7                       GOTO   LOOP
                                                    
                                                    END


MEMORY USAGE MAP ('X' = Used,  '-' = Unused)

0000 : XXXXXXXXXXXXXXXX XXXX------------ ---------------- ----------------

All other memory blocks unused.

Program Memory Words Used:    10

