gplink-2.1.3 (Mar 12 2018)
Listing File Generated: 2018-5-14  11:03:31
 
 
Address  Value    Disassembly              Source
-------  -----    -----------              ------
                                           #include "mc32p21.inc"
                                           		LIST
                                           ;mc32p21.inc    Standard Header File, Version 1.00 by Sinomcu
                                           		NOLIST
                                           
                                           
                                           
                                              	org 0x00
                                           start:
000000   3caa     movai   0xaa                	movai  	0xaa
000001   5610     movra   0x10                	movra  	0x10
000002   3c08     movai   0x8                      movai  	low(table)
000003   5784     movra   0x184                    movra  	FSR0
000004   3c00     movai   0                        movai  	high(table)
000005   5785     movra   0x185                    movra  	FSR1
                                           loop:
000006   6610     incr    0x10                	incr   	0x10
000007   a006     goto    0x6                 	goto   	loop
                                                  
                                           table:       
000008   aa55     goto    0xa55                dw  0xaa55,0x33,0x77;
000009   0033     dw      0x33             
00000a   0077     dw      0x77             
00000b   3388     dw      0x3388               db 	0x33,0x88;
                                              	
                                           
                                              	end       


MEMORY USAGE MAP ('X' = Used,  '-' = Unused)

0000 : XXXXXXXXXXXXXXXX XXXXXXXX-------- ---------------- ----------------

All other memory blocks unused.

Program Memory Words Used:    12

